# Vehicle sampling checklist OD-C (charter)

|  |  |
| --- | --- |
| Plate number: | Frontline reference for vehicle stop: |
| **Item** | **Details** | **Compliant (C) Non-complaint (NC), or N/A** | **Officer comments (include details of any notices issued)** |
| Vehicle is registered |  |  |
| Vehicle is authorised |  |  |
| Vehicle meets *Road Traffic (Vehicle) Regulations 2014* and applicable Australian Design Rule standards | All tyres meet required standard. |  |  |
| Seatbelts are free from defects and operate as required |  |
| Bodywork is free from any damage which could be unsafe |  |
| Fire extinguishers have been inspected in the last 6 months (vehicles with 10 or more seats, including driver, only) |  |
| First aid kit is fitted: Only applies to Omnibus vehicle equipped to seat more than 8 persons or operating on a route most of which lies outside the metropolitan region (r.386) |  |
| Camera Surveillance Unit  | If Camera Surveillance Unit is present (any type) Signage notifying passenger of use of recording device is present in front of vehicle in view of passengers (internal only) |  |  |
| Signage and Livery | * Does not resemble a taxi or display the word Taxi or words with similar meaning
 |  |  |
| * When operating, the vehicle displays either:
	+ Prominent livery for the booking service, or
	+ A sign clearly visible from the outside and positioned on the left of the rear window or otherwise clearly visible from the rear (day and night), and containing the ODBS name or logo.
 |  |